05-15 15:41:51.569: E/Sensors(143): LightSensor: event (type=3, code=40,mPendingEvent.light=180.000000,RAWvalue=83)

05-15 15:41:53.169: E/Sensors(143): LightSensor: event (type=3, code=40,mPendingEvent.light=180.000000,RAWvalue=68)

05-15 15:41:53.859: I/IdleService(143): next timeout 1000 msec from now

05-15 15:41:53.859: I/IdleService(143): SetTimerExpiryIfBefore: next timeout 1000 msec from now

05-15 15:41:53.859: I/IdleService(143): reset timer expiry to 1009 msec from now

05-15 15:41:53.859: I/IdleService(143): Reset idle timeout: tell observer 4783c6f0 user is back

05-15 15:41:54.869: I/IdleService(143): Get idle time: time since reset 879 msec

05-15 15:41:54.869: I/IdleService(143): Idle timer callback: current idle time 879 msec

05-15 15:41:54.869: I/IdleService(143): next timeout 120 msec from now

05-15 15:41:54.869: I/IdleService(143): SetTimerExpiryIfBefore: next timeout 120 msec from now

05-15 15:41:54.869: I/IdleService(143): reset timer expiry to 129 msec from now

05-15 15:41:55.009: I/IdleService(143): Get idle time: time since reset 1015 msec

05-15 15:41:55.009: I/IdleService(143): Idle timer callback: current idle time 1015 msec

05-15 15:41:55.009: I/IdleService(143): next timeout 4294967293984 msec from now

05-15 15:41:55.009: I/IdleService(143): SetTimerExpiryIfBefore: next timeout 4294967293983 msec from now

05-15 15:41:55.009: I/IdleService(143): reset timer expiry to 4294967293992 msec from now

05-15 15:41:55.009: I/IdleService(143): Idle timer callback: tell observer 4783c6f0 user is idle

05-15 15:41:55.009: I/IdleService(143): Get idle time: time since reset 1018 msec

05-15 15:41:55.579: I/Diag\_Lib(147): rpc\_handle\_rpc\_call: for Xid: 222, Prog: 31000000, Vers: d17ed9ea, Proc: 00000014

05-15 15:41:55.579: I/Diag\_Lib(147): rpc\_handle\_rpc\_call: Find Status: 0 Xid: 222

05-15 15:41:55.589: D/QCRIL\_RPC(147): Enter qcril\_cm\_srvsys\_event\_callback

05-15 15:41:55.589: D/QCRIL\_RPC(147): Exit qcril\_cm\_srvsys\_event\_callback

05-15 15:41:55.589: D/SST\_QC\_B2G(143): Signal Strength changed; sending info to content process

05-15 15:41:55.589: D/SIGNAL\_STRENGTH\_QC\_B2G(143): GetDbm = -79

05-15 15:41:55.589: D/SIGNAL\_STRENGTH\_QC\_B2G(143): GetRelSignalStrength = 54

05-15 15:41:55.589: D/SIGNAL\_STRENGTH\_QC\_B2G(143): GetDbm = -79

05-15 15:41:55.589: D/SIGNAL\_STRENGTH\_QC\_B2G(143): GetRelSignalStrength = 54

05-15 15:41:55.589: I/Gecko(143): -\*- QCContentHelper\_QC\_B2G: sendMessage to content process: RIL:VoiceInfoChanged{connected : true,emergencyCallsOnly : false,roaming : false,type : 'hspa',signalStrength : -79,relSignalStrength : 54,network : {mcc : '310', mnc : '410', longName : 'AT&T', shortName : 'AT&T'},cell : {gsmLocationAreaCode : 42980, gsmCellId :9407291},state : 'registered'}

05-15 15:41:55.589: I/ONCRPC(147): oncrpc\_proxy\_handle\_cmd\_rpc\_call: Dispatching xid: 222

05-15 15:41:55.589: I/ONCRPC(147): oncrpc\_xdr\_reply\_msg\_start: Prog: 00000000, Ver: 00000000, Proc: 00000000 Xid: 00000222

05-15 15:41:55.589: I/ONCRPC(147): oncrpc\_msg\_reply: Prog: 00000000, Ver: 00000000, Proc: 00000000 Xid: 00000222

05-15 15:41:55.589: I/ONCRPC(147): oncrpc\_proxy\_handle\_cmd\_rpc\_call: Dispatch returned for xid: 222

05-15 15:41:55.599: I/Gecko(143): -\*- QCContentHelper\_QC\_B2G: sendMessage to content process: RIL:DataInfoChanged{connected : true,emergencyCallsOnly : false,roaming : false,type : 'hspa',signalStrength : -79,relSignalStrength : 54,network : {mcc : '310', mnc : '410', longName : 'AT&T', shortName : 'AT&T'},cell : {gsmLocationAreaCode : 42980, gsmCellId :9407291},state : 'registered'}

05-15 15:42:00.299: E/Sensors(143): LightSensor: event (type=3, code=40,mPendingEvent.light=180.000000,RAWvalue=79)

05-15 15:42:00.559: E/Sensors(143): LightSensor: event (type=3, code=40,mPendingEvent.light=320.000000,RAWvalue=183)

05-15 15:42:00.719: E/Sensors(143): LightSensor: event (type=3, code=40,mPendingEvent.light=800.000000,RAWvalue=366)

05-15 15:42:01.129: E/Sensors(143): LightSensor: event (type=3, code=40,mPendingEvent.light=490.000000,RAWvalue=304)

05-15 15:42:01.439: E/Sensors(143): LightSensor: event (type=3, code=40,mPendingEvent.light=800.000000,RAWvalue=545)

05-15 15:42:01.799: E/Sensors(143): LightSensor: event (type=3, code=40,mPendingEvent.light=1500.000000,RAWvalue=846)

05-15 15:42:07.579: I/Diag\_Lib(147): rpc\_handle\_rpc\_call: for Xid: 227, Prog: 31000000, Vers: d17ed9ea, Proc: 00000014